# Method smoothers_uild

[ next ] [ prev ] [ prev-tail ] [ tail ] [ up ]

#### 5.4 Method smoothers_build

`call p%smoothers_build(a,desc_a,p,info[,amold,vmold,imold])`

This method builds the smoothers and the coarsest-level solvers for the multilevel preconditioner `p`, according to the requirements made by the user through the methods `init` and `set`, and based on the aggregation hierarchy produced by a previous call to `hierarchy_build` (see Section 5.3 ).

Arguments

`a` | `type(psb_`x `spmat_type), intent(in)`.
| The sparse matrix structure containing the local part of the matrix to be preconditioned. Note that x must be chosen according to the `real`/`complex`, single/double precision version of AMG4PSBLAS under use. See the PSBLAS User’s Guide for details [ 21 ].
`desc_a` | `type(psb_desc_type), intent(in)`.
| The communication descriptor of `a`. See the PSBLAS User’s Guide for details [ 21 ].
`info` | `integer, intent(out)`.
| Error code. If no error, 0 is returned. See Section 7 for details.
`amold` | `class(psb_`x`_base_sparse_mat), intent(in), optional`.
| The desired dynamic type for internal matrix components; this allows e.g. running on GPUs; it needs not be the same on all processes. See the PSBLAS User’s Guide for details [ 21 ].
`vmold` | `class(psb_`x`_base_vect_type), intent(in), optional`.
| The desired dynamic type for internal vector components; this allows e.g. running on GPUs.
`imold` | `class(psb_i_base_vect_type), intent(in), optional`.
| The desired dynamic type for internal integer vector components; this allows e.g. running on GPUs.

[ next ] [ prev ] [ prev-tail ] [ front ] [ up ]