# psb_geasb — Assembly a dense matrix

[next] [prev] [prev-tail] [tail] [up]

#### 6.14 psb_geasb — Assembly a dense matrix

    call psb_geasb(x, desc_a, info, mold)

Type:
  Synchronous.
On Entry
desc_a
  The communication descriptor.
  Scope: local
  Type: required
  Intent: in.
  Specified as: a variable of type psb_desc_type.
mold
  The desired dynamic type for the internal vector storage.
  Scope: local.
  Type: optional.
  Intent: in.
  Specified as: an object of a class derived from psb_T_base_vect_type; this is only allowed when x is of type psb_T_vect_type.

On Return
x
  The dense matrix to be assembled.
  Scope: local
  Type: required
  Intent: inout.
  Specified as: a rank one or two array with the ALLOCATABLE or an object of type psb_T_vect_type, of type real, complex or integer.
info
  Error code.
  Scope: local
  Type: required
  Intent: out.
  An integer value; 0 means no error has been detected.

Notes

1. On entry to this routine the descriptor must be in the assembled state, i.e. psb_cdasb must already have been called.
2. If the bldmode=psb_matbld_remote_ value was specified at allocation time, contributions defined on the current process but belonging to a remote process will be handled accordingly. This is most likely to occur in finite element applications, with dupl=psb_dupl_add_.

[next] [prev] [prev-tail] [front] [up]